<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN"
    "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<html xmlns="http://www.w3.org/1999/xhtml">
  <head>
    <meta name="generator" content="HTML Tidy, see www.w3.org" />

    <title>Stopping and Restarting the Server</title>
  </head>
  <!-- Background white, links blue (unvisited), navy (visited), red (active) -->

  <body bgcolor="#FFFFFF" text="#000000" link="#0000FF"
  vlink="#000080" alink="#FF0000">
        <div align="center">
      <img src="images/sub.gif" alt="[APACHE DOCUMENTATION]" /> 

      <h3>Apache HTTP Server Version 2.0</h3>
    </div>




    <h1 align="center">Stopping and Restarting the Server</h1>

    <p>This document covers stopping and restarting Apache on
    Unix-like systems. Windows users should see <a
    href="platform/windows.html#signal">Signalling Apache when
    running</a>.</p>

    <p>You will notice many <code>httpd</code> executables running
    on your system, but you should not send signals to any of them
    except the parent, whose pid is in the <a
    href="mod/mpm_common.html#pidfile">PidFile</a>. That is to say you
    shouldn't ever need to send signals to any process except the
    parent. There are three signals that you can send the parent:
    <code>TERM</code>, <code>HUP</code>, and <code>USR1</code>,
    which will be described in a moment.</p>

    <p>To send a signal to the parent you should issue a command
    such as:</p>

    <blockquote>
<pre>
    kill -TERM `cat /usr/local/apache/logs/httpd.pid`
</pre>
    </blockquote>
    You can read about its progress by issuing: 

    <blockquote>
<pre>
    tail -f /usr/local/apache/logs/error_log
</pre>
    </blockquote>
    Modify those examples to match your <a
    href="mod/core.html#serverroot">ServerRoot</a> and <a
    href="mod/mpm_common.html#pidfile">PidFile</a> settings. 

    <p>A shell script called <a
    href="programs/apachectl.html">apachectl</a> is provided which
    automates the processing of signalling Apache. For details
    about this script, see the documentation on <a
    href="invoking.html">starting Apache</a>.</p>

    <h3>Stop Now</h3>

    <p><strong>Signal:</strong> TERM<br />
     <code>apachectl stop</code></p>

    <p>Sending the <code>TERM</code> signal to the parent causes it
    to immediately attempt to kill off all of its children. It may
    take it several seconds to complete killing off its children.
    Then the parent itself exits. Any requests in progress are
    terminated, and no further requests are served.</p>

    <h3>Graceful Restart</h3>

    <p><strong>Signal:</strong> USR1<br />
     <code>apachectl graceful</code></p>

    <p>The <code>USR1</code> signal causes the parent process to
    <em>advise</em> the children to exit after their current
    request (or to exit immediately if they're not serving
    anything). The parent re-reads its configuration files and
    re-opens its log files. As each child dies off the parent
    replaces it with a child from the new <em>generation</em> of
    the configuration, which begins serving new requests
    immediately.</p>
    <i>On certain platforms that do not allow USR1 to be used for a
    graceful restart, an alternative signal may be used (such as
    WINCH). apachectl graceful will send the right signal for your
    platform.</i> 

    <p>This code is designed to always respect the <a
    href="mod/mpm_common.html#maxclients">MaxClients</a>, <a
    href="mod/prefork.html#minspareservers">MinSpareServers</a>,
    and <a
    href="mod/prefork.html#maxspareservers">MaxSpareServers</a>
    settings. Furthermore, it respects <a
    href="mod/mpm_common.html#startservers">StartServers</a> in the
    following manner: if after one second at least StartServers new
    children have not been created, then create enough to pick up
    the slack. This is to say that the code tries to maintain both
    the number of children appropriate for the current load on the
    server, and respect your wishes with the StartServers
    parameter.</p>

    <p>Users of the <a href="mod/mod_status.html">status module</a>
    will notice that the server statistics are <strong>not</strong>
    set to zero when a <code>USR1</code> is sent. The code was
    written to both minimize the time in which the server is unable
    to serve new requests (they will be queued up by the operating
    system, so they're not lost in any event) and to respect your
    tuning parameters. In order to do this it has to keep the
    <em>scoreboard</em> used to keep track of all children across
    generations.</p>

    <p>The status module will also use a <code>G</code> to indicate
    those children which are still serving requests started before
    the graceful restart was given.</p>

    <p>At present there is no way for a log rotation script using
    <code>USR1</code> to know for certain that all children writing
    the pre-restart log have finished. We suggest that you use a
    suitable delay after sending the <code>USR1</code> signal
    before you do anything with the old log. For example if most of
    your hits take less than 10 minutes to complete for users on
    low bandwidth links then you could wait 15 minutes before doing
    anything with the old log.</p>

    <p><strong>Note:</strong> If your configuration file has errors
    in it when you issue a restart then your parent will not
    restart, it will exit with an error. In the case of graceful
    restarts it will also leave children running when it exits.
    (These are the children which are "gracefully exiting" by
    handling their last request.) This will cause problems if you
    attempt to restart the server -- it will not be able to bind to
    its listening ports. Before doing a restart, you can check the
    syntax of the configuration files with the <code>-t</code>
    command line argument (see <a
    href="programs/httpd.html">httpd</a>). This still will not
    guarantee that the server will restart correctly. To check the
    semantics of the configuration files as well as the syntax, you
    can try starting httpd as a non-root user. If there are no
    errors it will attempt to open its sockets and logs and fail
    because it's not root (or because the currently running httpd
    already has those ports bound). If it fails for any other
    reason then it's probably a config file error and the error
    should be fixed before issuing the graceful restart.</p>

    <h3>Restart Now</h3>

    <p><strong>Signal:</strong> HUP<br />
     <code>apachectl restart</code></p>

    <p>Sending the <code>HUP</code> signal to the parent causes it
    to kill off its children like in <code>TERM</code> but the
    parent doesn't exit. It re-reads its configuration files, and
    re-opens any log files. Then it spawns a new set of children
    and continues serving hits.</p>

    <p>Users of the <a href="mod/mod_status.html">status module</a>
    will notice that the server statistics are set to zero when a
    <code>HUP</code> is sent.</p>

    <p><strong>Note:</strong> If your configuration file has errors
    in it when you issue a restart then your parent will not
    restart, it will exit with an error. See below for a method of
    avoiding this.</p>

    <h3>Appendix: signals and race conditions</h3>

    <p>Prior to Apache 1.2b9 there were several <em>race
    conditions</em> involving the restart and die signals (a simple
    description of race condition is: a time-sensitive problem, as
    in if something happens at just the wrong time it won't behave
    as expected). For those architectures that have the "right"
    feature set we have eliminated as many as we can. But it should
    be noted that there still do exist race conditions on certain
    architectures.</p>

    <p>Architectures that use an on disk <a
    href="mod/mpm_common.html#scoreboardfile">ScoreBoardFile</a> have the
    potential to corrupt their scoreboards. This can result in the
    "bind: Address already in use" (after <code>HUP</code>) or
    "long lost child came home!" (after <code>USR1</code>). The
    former is a fatal error, while the latter just causes the
    server to lose a scoreboard slot. So it might be advisable to
    use graceful restarts, with an occasional hard restart. These
    problems are very difficult to work around, but fortunately
    most architectures do not require a scoreboard file. See the <a
    href="mod/mpm_common.html#scoreboardfile">ScoreBoardFile</a>
    documentation for a architecture uses it.</p>

    <p><code>NEXT</code> and <code>MACHTEN</code> (68k only) have
    small race conditions which can cause a restart/die signal to
    be lost, but should not cause the server to do anything
    otherwise problematic. 
    <!-- they don't have sigaction, or we're not using it -djg -->
    </p>

    <p>All architectures have a small race condition in each child
    involving the second and subsequent requests on a persistent
    HTTP connection (KeepAlive). It may exit after reading the
    request line but before reading any of the request headers.
    There is a fix that was discovered too late to make 1.2. In
    theory this isn't an issue because the KeepAlive client has to
    expect these events because of network latencies and server
    timeouts. In practice it doesn't seem to affect anything either
    -- in a test case the server was restarted twenty times per
    second and clients successfully browsed the site without
    getting broken images or empty documents. </p>
        <hr />

    <h3 align="center">Apache HTTP Server Version 2.0</h3>
    <a href="./"><img src="images/index.gif" alt="Index" /></a>



  </body>
</html>

