<?xml version="1.0" encoding="UTF-8" ?>
<!DOCTYPE manualpage SYSTEM "./style/manualpage.dtd">
<?xml-stylesheet type="text/xsl" href="./style/manual.en.xsl"?>
<!-- $Revision: 1.2.2.8 $ -->

<!--
 Copyright 2002-2004 The Apache Software Foundation

 Licensed under the Apache License, Version 2.0 (the "License");
 you may not use this file except in compliance with the License.
 You may obtain a copy of the License at

     http://www.apache.org/licenses/LICENSE-2.0

 Unless required by applicable law or agreed to in writing, software
 distributed under the License is distributed on an "AS IS" BASIS,
 WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
 See the License for the specific language governing permissions and
 limitations under the License.
-->

<manualpage metafile="bind.xml.meta">

  <title>Binding</title>

  <summary>
    <p>Configuring Apache to listen on specific addresses and ports.</p>
  </summary>

  <seealso><a href="vhosts/">Virtual Hosts</a></seealso>
  <seealso><a href="dns-caveats.html">DNS Issues</a></seealso>

  <section id="overview">
    <title>Overview</title>

    <related>
      <modulelist>
        <module>core</module>
        <module>mpm_common</module>
      </modulelist>
      <directivelist>
        <directive module="core" type="section">VirtualHost</directive>
        <directive module="mpm_common">Listen</directive>
      </directivelist>
    </related>


    <p>When Apache starts, it binds to some port and address on
    the local machine and waits for incoming requests. By default,
    it listens to all addresses on the machine.  However, it needs to
    be told to listen on specific ports, or to listen on only selected 
    addresses, or a combination. This is often combined with the 
    Virtual Host feature which determines how Apache responds to 
    different IP addresses, hostnames and ports.</p>

    <p>The <directive module="mpm_common">Listen</directive>
    directive tells the server to accept
    incoming requests only on the specified port or
    address-and-port combinations. If only a port number is
    specified in the <directive module="mpm_common">Listen</directive>
    directive, the server
    listens to the given port on all interfaces. If an IP address
    is given as well as a port, the server will listen on the given
    port and interface. Multiple Listen directives may be used to
    specify a number of addresses and ports to listen on. The
    server will respond to requests from any of the listed
    addresses and ports.</p>

    <p>For example, to make the server accept connections on both
    port 80 and port 8000, use:</p>

    <example>
      Listen 80<br />
      Listen 8000
    </example>

    <p>To make the server accept connections on two specified
    interfaces and port numbers, use</p>

    <example>
      Listen 192.170.2.1:80<br />
      Listen 192.170.2.5:8000
    </example>

    <p>IPv6 addresses must be surrounded in square brackets, as in the
    following example:</p>

    <example>
      Listen [fe80::a00:20ff:fea7:ccea]:80
    </example>
  </section>

  <section id="ipv6">
    <title>Special IPv6 Considerations</title>

    <p>A growing number of platforms implement IPv6, and APR supports 
    IPv6 on most of these platforms, allowing Apache to allocate IPv6 
    sockets and handle requests which were sent over IPv6.</p>

    <p>One complicating factor for Apache administrators is whether or
    not an IPv6 socket can handle both IPv4 connections and IPv6 
    connections.  Handling IPv4 connections with an IPv6 socket uses 
    IPv4-mapped IPv6 addresses, which are allowed by default on most 
    platforms but are disallowed by default on FreeBSD, NetBSD, and 
    OpenBSD in order to match the system-wide policy on those
    platforms.  But even on systems where it is disallowed by default, a 
    special configure parameter can change this behavior for Apache.</p>

    <p>If you want Apache to handle IPv4 and IPv6 connections with a 
    minimum of sockets, which requires using IPv4-mapped IPv6 addresses, 
    specify the <code>--enable-v4-mapped</code> configure option and use 
    generic Listen directives like the following:</p>

    <example>
      Listen 80
    </example>

    <p>With <code>--enable-v4-mapped</code>, the Listen directives in the 
    default configuration file created by Apache will use this form.  
    <code>--enable-v4-mapped</code> is the default on all platforms but 
    FreeBSD, NetBSD, and OpenBSD, so this is probably how your Apache was 
    built.</p>

    <p>If you want Apache to handle IPv4 connections only, regardless of 
    what your platform and APR will support, specify an IPv4 address on all 
    Listen directives, as in the following examples:</p>

    <example>
      Listen 0.0.0.0:80<br />
      Listen 192.170.2.1:80
    </example>

    <p>If you want Apache to handle IPv4 and IPv6 connections on separate 
    sockets (i.e., to disable IPv4-mapped addresses), specify the 
    <code>--disable-v4-mapped</code> configure option and use specific Listen 
    directives like the following:</p>

    <example>
      Listen [::]:80<br />
      Listen 0.0.0.0:80
    </example>

    <p>With <code>--disable-v4-mapped</code>, the Listen directives in the 
    default configuration file created by Apache will use this form.  
    <code>--disable-v4-mapped</code> is the default on FreeBSD, NetBSD, and 
    OpenBSD.</p>

  </section>

  <section id="virtualhost">
    <title>How This Works With Virtual Hosts</title>

    <p>Listen does not implement Virtual Hosts. It only tells the
    main server what addresses and ports to listen to. If no
    <directive module="core" type="section">VirtualHost</directive>
    directives are used, the server will behave
    the same for all accepted requests. However,
    <directive module="core" type="section">VirtualHost</directive>
    can be used to specify a different behavior
    for one or more of the addresses and ports. To implement a
    VirtualHost, the server must first be told to listen to the
    address and port to be used. Then a
    <directive module="core" type="section">VirtualHost</directive> section
    should be created for a specified address and port to set the
    behavior of this virtual host. Note that if the
    <directive module="core" type="section">VirtualHost</directive>
    is set for an address and port that the
    server is not listening to, it cannot be accessed.</p>
  </section>
</manualpage>

